<< cmd_arduino_d_control | Arduino toolbox | cmd_dcmotor_release >>

Arduino toolbox >> Arduino toolbox > cmd_arduino_meter

# cmd_arduino_meter

GUI to display continuous signal from a loop, and break the loop after termination of the GUI

### Calling Sequence

    cmd_arduino_meter(val)

### Parameters

val :

  Value to be displayed

### Description

This GUI provides a convenient way display a continuous data from a loop and break the loop after the termination of the GUI. By this, it behave like a digital meter by showing the data in a GUI instead of the console

### Examples

    ok = open_serial(1,9,115200)
    val = cmd_analog_in_volt(1,9)
    cmd_arduino_meter(val)
    close_serial(1)

### See also

- cmd_arduino_d_control
- cmd_arduino_a_control

### Authors

- Bruno JOFRET, Tan C.L.

Report an issue
<< cmd_arduino_d_control | Arduino toolbox | cmd_dcmotor_release >>