<< cmd_arduino_a_control | Arduino toolbox | cmd_arduino_meter >>

Arduino toolbox >> Arduino toolbox > cmd_arduino_d_control

# cmd_arduino_d_control

GUI to control digital signal to be sent to a connected Arduino board

### Calling Sequence

    cmd_arduino_d_control(h,pin_no)

### Parameters

h :

  Board number, reserved for future use. For this version, any number would do

pin_no :

  Digital pin to sent the signal

### Description

This GUI provides a convenient way to control the value (0-255) to sent to the given pin number on Arduino.

### Examples

    ok = open_serial(1,9,115200)
    cmd_arduino_d_control(1,9)
    close_serial(1)

### See also

- cmd_digital_out_volt
- cmd_digital_out

### Authors

- Bruno JOFRET, Tan C.L.
- str = string(val)

Report an issue
<< cmd_arduino_a_control | Arduino toolbox | cmd_arduino_meter >>