(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 201)
    (zones 0)
    (modules 25)
    (nets 36)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 V+)
  (net 5 "Net-(JP1-Pad8)")
  (net 6 /IR1.1)
  (net 7 "Net-(JP1-Pad4)")
  (net 8 "Net-(JP1-Pad3)")
  (net 9 "Net-(JP1-Pad2)")
  (net 10 /IR1.2)
  (net 11 /IR2.1)
  (net 12 /IR2.2)
  (net 13 "Net-(JP2-Pad6)")
  (net 14 "Net-(JP2-Pad5)")
  (net 15 "Net-(JP2-Pad4)")
  (net 16 "Net-(JP2-Pad3)")
  (net 17 "Net-(JP2-Pad2)")
  (net 18 "Net-(JP2-Pad1)")
  (net 19 "Net-(JP3-Pad6)")
  (net 20 "Net-(JP4-Pad6)")
  (net 21 "Net-(JP4-Pad5)")
  (net 22 "Net-(JP4-Pad4)")
  (net 23 "Net-(JP4-Pad2)")
  (net 24 "Net-(JP4-Pad1)")
  (net 25 "Net-(R3-Pad1)")
  (net 26 "Net-(R1-Pad1)")
  (net 27 "Net-(R2-Pad1)")
  (net 28 "Net-(D1-PadA)")
  (net 29 "Net-(R9-Pad2)")
  (net 30 "Net-(BUTTON1-Pad1)")
  (net 31 "Net-(HALL1-PadOUT)")
  (net 32 "Net-(RELAY1-Pad3)")
  (net 33 "Net-(RELAY1-Pad6)")
  (net 34 "Net-(RELAY1-Pad1)")
  (net 35 "Net-(PIEZO1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /IR1.1)
    (add_net /IR1.2)
    (add_net /IR2.1)
    (add_net /IR2.2)
    (add_net GND)
    (add_net "Net-(BUTTON1-Pad1)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(HALL1-PadOUT)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP1-Pad3)")
    (add_net "Net-(JP1-Pad4)")
    (add_net "Net-(JP1-Pad8)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP2-Pad3)")
    (add_net "Net-(JP2-Pad4)")
    (add_net "Net-(JP2-Pad5)")
    (add_net "Net-(JP2-Pad6)")
    (add_net "Net-(JP3-Pad6)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP4-Pad4)")
    (add_net "Net-(JP4-Pad5)")
    (add_net "Net-(JP4-Pad6)")
    (add_net "Net-(PIEZO1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(RELAY1-Pad1)")
    (add_net "Net-(RELAY1-Pad3)")
    (add_net "Net-(RELAY1-Pad6)")
    (add_net V+)
  )
  (module shield-V1p2:1X08 (layer Top) (tedit 0)
    (at 143.6751 81.0006 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP1 (at -10.2362 -1.8288 180) (layer F.SilkS) hide)
    (fp_text value PINHD-1X8 (at -10.16 3.175) (layer F.Fab))
    (pad 8 thru_hole oval (at 8.89 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(JP1-Pad8)") (solder_mask_margin 0.0508))
    (pad 7 thru_hole oval (at 6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole oval (at 3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /IR1.1) (solder_mask_margin 0.0508))
    (pad 5 thru_hole oval (at 1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(BUTTON1-Pad1)") (solder_mask_margin 0.0508))
    (pad 4 thru_hole oval (at -1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(JP1-Pad4)") (solder_mask_margin 0.0508))
    (pad 3 thru_hole oval (at -3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(JP1-Pad3)") (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at -6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(JP1-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -8.89 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /IR1.2) (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:1X08 (layer Top) (tedit 0)
    (at 165.3921 81.0006 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP2 (at -10.2362 -1.8288 180) (layer F.SilkS) hide)
    (fp_text value PINHD-1X8 (at -10.16 3.175) (layer F.Fab))
    (pad 8 thru_hole oval (at 8.89 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /IR2.1) (solder_mask_margin 0.0508))
    (pad 7 thru_hole oval (at 6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /IR2.2) (solder_mask_margin 0.0508))
    (pad 6 thru_hole oval (at 3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(JP2-Pad6)") (solder_mask_margin 0.0508))
    (pad 5 thru_hole oval (at 1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(JP2-Pad5)") (solder_mask_margin 0.0508))
    (pad 4 thru_hole oval (at -1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(JP2-Pad4)") (solder_mask_margin 0.0508))
    (pad 3 thru_hole oval (at -3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(JP2-Pad3)") (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at -6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(JP2-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -8.89 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(JP2-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:1X06 (layer Top) (tedit 0)
    (at 150.1521 129.1336 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP3 (at -7.6962 -1.8288 180) (layer F.SilkS) hide)
    (fp_text value PINHD-1X6 (at -7.62 3.175) (layer F.Fab))
    (pad 6 thru_hole oval (at 6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(JP3-Pad6)") (solder_mask_margin 0.0508))
    (pad 5 thru_hole oval (at 3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3) (solder_mask_margin 0.0508))
    (pad 4 thru_hole oval (at 1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad 3 thru_hole oval (at -1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at -3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 V+) (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:1X06 (layer Top) (tedit 0)
    (at 168.0591 129.2606 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP4 (at -7.6962 -1.8288 180) (layer F.SilkS) hide)
    (fp_text value PINHD-1X6 (at -7.62 3.175) (layer F.Fab))
    (pad 6 thru_hole oval (at 6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(JP4-Pad6)") (solder_mask_margin 0.0508))
    (pad 5 thru_hole oval (at 3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(JP4-Pad5)") (solder_mask_margin 0.0508))
    (pad 4 thru_hole oval (at 1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(JP4-Pad4)") (solder_mask_margin 0.0508))
    (pad 3 thru_hole oval (at -1.27 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(HALL1-PadOUT)") (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at -3.81 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(JP4-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -6.35 0 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(JP4-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:B3F-10XX (layer Top) (tedit 0)
    (at 129.9591 92.6846 270)
    (descr "<b>OMRON SWITCH</b>")
    (fp_text reference BUTTON1 (at 3.302 4.445 90) (layer F.SilkS))
    (fp_text value 10-XX (at -3.048 5.08 90) (layer F.Fab))
    (fp_text user 4 (at 3.556 2.794 270) (layer F.Fab))
    (fp_text user 3 (at -4.572 2.794 270) (layer F.Fab))
    (fp_text user 2 (at 3.556 -1.524 270) (layer F.Fab))
    (fp_text user 1 (at -4.318 -1.651 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.2512 2.2606 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at 3.2512 -2.2606 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(BUTTON1-Pad1)") (solder_mask_margin 0.0508))
    (pad 3 thru_hole oval (at -3.2512 2.2606 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -3.2512 -2.2606 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(BUTTON1-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 134.4041 100.8126 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R6 (at 8.382 -0.762) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "Net-(BUTTON1-Pad1)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:RGB_VERTICAL (layer Top) (tedit 0)
    (at 128.8161 81.5086)
    (fp_text reference RGB1 (at -3.683 2.286 90) (layer F.SilkS))
    (fp_text value "RGB LED" (at 3.175 3.81) (layer F.Fab))
    (pad 4 thru_hole circle (at -1.905 0 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R3-Pad1)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at 3.81 0 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R1-Pad1)") (solder_mask_margin 0.0508))
    (pad 2 thru_hole rect (at 1.905 0 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R2-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 139.8651 85.3186)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R1 (at 6.096 0.254) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(JP1-Pad4)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "Net-(R1-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 139.8651 88.1126)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R2 (at 6.096 0.254) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(JP1-Pad3)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(R2-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 139.8651 90.7796)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R3 (at 6.096 0.254) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(JP1-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "Net-(R3-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:VERT_POT (layer Top) (tedit 0)
    (at 134.0231 117.1956 180)
    (fp_text reference POT1 (at 7.056 -0.452) (layer F.SilkS))
    (fp_text value EVU_POTENTIOMETER (at 0 0 180) (layer F.SilkS) hide)
    (pad P$5 thru_hole rect (at 4.5 -7 180) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad P$4 thru_hole rect (at -4.5 -7 180) (size 3.81 3.81) (drill 2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -2.5 0 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 thru_hole circle (at 2.5 0 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(JP4-Pad4)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:TO_92_SHORT (layer Top) (tedit 0)
    (at 123.3551 128.2446 90)
    (fp_text reference HALL1 (at 2.032 -3.048 90) (layer F.SilkS))
    (fp_text value SS49E (at 0 0 90) (layer F.SilkS) hide)
    (pad V+ thru_hole oval (at -1.905 0 180) (size 2.016 1.008) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad OUT thru_hole oval (at 1.905 0 180) (size 2.016 1.008) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(HALL1-PadOUT)") (solder_mask_margin 0.0508))
    (pad V- thru_hole oval (at 0 0 180) (size 2.016 1.008) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:TSC_RELAY (layer Top) (tedit 0)
    (at 161.3281 95.8596 270)
    (fp_text reference RELAY1 (at -2.794 5.334 90) (layer F.SilkS))
    (fp_text value TSC_1FORMC (at 0 0 270) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 5.08 -2.54 270) (size 1.6764 1.6764) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(RELAY1-Pad3)") (solder_mask_margin 0.0508))
    (pad 4 thru_hole circle (at 5.08 2.54 270) (size 1.6764 1.6764) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(RELAY1-Pad3)") (solder_mask_margin 0.0508))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 1.6764 1.6764) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad 5 thru_hole circle (at -2.54 2.54 270) (size 1.6764 1.6764) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D1-PadA)") (solder_mask_margin 0.0508))
    (pad 6 thru_hole circle (at -5.08 2.54 270) (size 1.6764 1.6764) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(RELAY1-Pad6)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 -2.54 270) (size 1.6764 1.6764) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(RELAY1-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:R-5 (layer Top) (tedit 0)
    (at 122.0851 117.4496 90)
    (descr <b>VARISTOR</b>)
    (fp_text reference THERM1 (at -3.048 2.54 90) (layer F.SilkS))
    (fp_text value Thermistor (at -2.54 2.286 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(JP4-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 134.4041 109.9566)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R7 (at -8.128 0.508) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(JP4-Pad2)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:TO46-VT200 (layer Top) (tedit 0)
    (at 122.3391 107.6706)
    (descr "<b>Photoconductive Cell</b> VT200 Series<p>\nSource: http://optoelectronics.perkinelmer.com/content/Datasheets/DTS_vt200seriesdatasheet.pdf")
    (fp_text reference PHOTO1 (at -2.3241 -2.8956 90) (layer F.SilkS))
    (fp_text value "CdS Photocell" (at -2.75 -3) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(JP4-Pad1)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 134.4041 106.9086)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R8 (at -8.128 0.508) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "Net-(JP4-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:TO92 (layer Top) (tedit 0)
    (at 153.0731 89.6366)
    (descr "<b>TO 92</b>")
    (fp_text reference T1 (at 0.381 3.175) (layer F.SilkS))
    (fp_text value 2N3904 (at 3.175 1.27) (layer F.Fab))
    (fp_text user 1 (at 1.143 0) (layer F.Fab))
    (fp_text user 3 (at -2.159 0) (layer F.Fab))
    (fp_text user 2 (at -0.635 -0.635) (layer F.Fab))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 2 thru_hole circle (at 0 -1.905) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(R9-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at 1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(D1-PadA)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:DO41-10 (layer Top) (tedit 0)
    (at 158.7881 104.2416 180)
    (descr "<B>DIODE</B><p>\ndiameter 2.54 mm, horizontal, grid 10.16 mm")
    (fp_text reference D1 (at 2.54 2.413) (layer F.SilkS))
    (fp_text value 1N4004 (at -2.032 2.794) (layer F.Fab))
    (pad C thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad A thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 28 "Net-(D1-PadA)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:W237-103 (layer Top) (tedit 0)
    (at 171.6151 97.0026 270)
    (descr "<b>WAGO SCREW CLAMP</b>")
    (fp_text reference X1 (at -7.7778 -1.4262) (layer F.SilkS))
    (fp_text value W237-103 (at -5.3048 4.9476 90) (layer F.Fab))
    (fp_text user 3 (at 3.1534 -0.615 270) (layer F.Fab))
    (fp_text user 2 (at -1.8504 -0.5642 270) (layer F.Fab))
    (fp_text user 1 (at -6.905 -0.615 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 1.29) (size 3.5814 1.7907) (drill 1.1938) (layers *.Cu *.Mask)
      (net 34 "Net-(RELAY1-Pad1)") (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at 0 1.29) (size 3.5814 1.7907) (drill 1.1938) (layers *.Cu *.Mask)
      (net 32 "Net-(RELAY1-Pad3)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -5 1.29) (size 3.5814 1.7907) (drill 1.1938) (layers *.Cu *.Mask)
      (net 33 "Net-(RELAY1-Pad6)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 164.1221 86.7156 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R9 (at 6.096 0.508) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(R9-Pad2)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(JP2-Pad3)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:0207_10 (layer Top) (tedit 0)
    (at 134.4041 103.8606)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R10 (at -9.144 0.508) (layer F.SilkS))
    (fp_text value R-US_0207_10 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(JP2-Pad4)") (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "Net-(PIEZO1-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:OSHW_FILLX150_NOTEXT (layer Top) (tedit 0)
    (at 166.2811 110.4646)
    (fp_text reference U$1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module shield-V1p2:PS1240P02BT (layer Top) (tedit 0)
    (at 149.0091 97.7646 270)
    (fp_text reference PIEZO1 (at -3.66 2.612) (layer F.SilkS))
    (fp_text value PS1240P02BT (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.9304 1.9304) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(PIEZO1-Pad1)") (solder_mask_margin 0.0508))
  )
  (module shield-V1p2:JP2 (layer Top) (tedit 0)
    (at 175.9331 109.4486 90)
    (descr <b>JUMPER</b>)
    (fp_text reference SERVO1 (at -3.556 -1.651 90) (layer F.SilkS))
    (fp_text value JP2E (at -3.556 4.318 90) (layer F.Fab))
    (fp_text user 3 (at 2.54 2.667 90) (layer F.SilkS))
    (fp_text user 2 (at 0 2.667 90) (layer F.SilkS))
    (fp_text user 1 (at -2.54 2.667 90) (layer F.SilkS))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.0508))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 "Net-(JP2-Pad6)") (solder_mask_margin 0.0508))
  )
  (gr_line (start 117.2591 132.3086) (end 179.7431 132.5626) (layer Edge.Cuts) (width 0.05))
  (gr_text RST (at 144.9552 131.0843) (layer F.SilkS))
  (gr_text 3v (at 147.2768 131.0285) (layer F.SilkS))
  (gr_text 5v (at 149.8168 131.0285) (layer F.SilkS))
  (gr_text Gnd (at 154.206 130.9929) (layer F.SilkS))
  (gr_text Vin (at 157.8178 131.0285) (layer F.SilkS))
  (gr_text 0 (at 162.334 131.1199) (layer F.SilkS))
  (gr_text 1 (at 164.874 131.1199) (layer F.SilkS))
  (gr_text 2 (at 167.414 131.1199) (layer F.SilkS))
  (gr_text 3 (at 169.954 131.1199) (layer F.SilkS))
  (gr_text 4 (at 172.494 131.1199) (layer F.SilkS))
  (gr_text 5 (at 174.907 131.1199) (layer F.SilkS))
  (gr_text 7 (at 157.1828 78.1965) (layer F.SilkS))
  (gr_text 6 (at 159.5958 78.1965) (layer F.SilkS))
  (gr_text 5 (at 162.2628 78.1965) (layer F.SilkS))
  (gr_text 4 (at 164.6504 78.2219) (layer F.SilkS))
  (gr_text 3 (at 167.0634 78.2473) (layer F.SilkS))
  (gr_text 2 (at 169.8066 78.1965) (layer F.SilkS))
  (gr_text 1 (at 172.4228 78.1711) (layer F.SilkS))
  (gr_text 0 (at 174.912 78.1711) (layer F.SilkS))
  (gr_text COM (at 177.2031 99.2886 90) (layer F.SilkS))
  (gr_text NO (at 177.2031 103.6066 90) (layer F.SilkS))
  (gr_text NC (at 176.6951 93.1926 90) (layer F.SilkS))
  (gr_text ARef (at 135.6842 78.1253) (layer F.SilkS))
  (gr_text gnd (at 138.7678 78.1965) (layer F.SilkS))
  (gr_text 13 (at 140.8506 78.1965) (layer F.SilkS))
  (gr_text 12 (at 143.3398 78.1965) (layer F.SilkS))
  (gr_text 11 (at 146.0576 78.1965) (layer F.SilkS))
  (gr_text 10 (at 148.5214 78.1965) (layer F.SilkS))
  (gr_text 9 (at 150.6042 78.1965) (layer F.SilkS))
  (gr_text 8 (at 153.1188 78.1965) (layer F.SilkS))
  (gr_text "Sensor Shield V-1.2" (at 141.6431 111.7346) (layer F.SilkS))
  (gr_line (start 179.7431 132.5626) (end 179.7431 77.6986) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.2591 77.4446) (end 179.7431 77.6986) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.2591 132.3086) (end 117.2591 77.4446) (layer Edge.Cuts) (width 0.05))
  (gr_text "Integrated Development Lab" (at 133.7691 114.5286) (layer F.SilkS))
  (gr_text "IIT Bombay" (at 150.5331 117.3226) (layer F.SilkS))
  (dimension 62.484516 (width 0.2) (layer Top)
    (gr_text "62.485 mm" (at 148.492466 75.532983 359.7670916) (layer Top))
    (feature1 (pts (xy 179.7431 73.536097) (xy 179.740213 74.246416)))
    (feature2 (pts (xy 117.2591 73.282097) (xy 117.256213 73.992416)))
    (crossbar (pts (xy 117.258596 73.406) (xy 179.742596 73.66)))
    (arrow1a (pts (xy 179.742596 73.66) (xy 178.613718 74.241837)))
    (arrow1b (pts (xy 179.742596 73.66) (xy 178.618485 73.069005)))
    (arrow2a (pts (xy 117.258596 73.406) (xy 118.382707 73.996995)))
    (arrow2b (pts (xy 117.258596 73.406) (xy 118.387474 72.824163)))
  )
  (dimension 54.864 (width 0.2) (layer Top)
    (gr_text "54.864 mm" (at 111.665 104.8766 270) (layer Top))
    (feature1 (pts (xy 113.665 132.3086) (xy 113.078579 132.3086)))
    (feature2 (pts (xy 113.665 77.4446) (xy 113.078579 77.4446)))
    (crossbar (pts (xy 113.665 77.4446) (xy 113.665 132.3086)))
    (arrow1a (pts (xy 113.665 132.3086) (xy 113.078579 131.182096)))
    (arrow1b (pts (xy 113.665 132.3086) (xy 114.251421 131.182096)))
    (arrow2a (pts (xy 113.665 77.4446) (xy 113.078579 78.571104)))
    (arrow2b (pts (xy 113.665 77.4446) (xy 114.251421 78.571104)))
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.3048)
    (fill yes (arc_segments 32) (thermal_gap 0.6596) (thermal_bridge_width 0.6596))
    (polygon
      (pts
        (xy 179.9209 77.395039) (xy 179.9209 132.868644) (xy 116.9543 132.612161) (xy 116.9543 77.138556)
      )
    )
  )
)
